WEBVTT

00:00.150 --> 00:03.470
Hello and welcome back to mastering Photoshop in this lesson.

00:03.480 --> 00:08.330
Let's have a look at different types of images or different file format for the images.

00:08.370 --> 00:15.150
Photoshop can understand or recognize open save and deal with several different types of file formats

00:15.570 --> 00:22.720
and to check that to go to a file and say open or control on your keyboard and hit the small drop down

00:22.770 --> 00:25.950
or all file formats and you see these many file formats.

00:25.950 --> 00:31.930
Photoshop can recognize or open or it can edit these types of images.

00:32.070 --> 00:34.120
We do not need to know all of them.

00:34.320 --> 00:41.820
And I tried to explain many of these file formats as we progressed through this course but we certainly

00:41.820 --> 00:43.830
do not need to know at this point of time.

00:43.830 --> 00:46.440
We do not need to know all of these file formats.

00:46.470 --> 00:53.520
We'll look at a couple of important file formats at this point of time so that we can start learning

00:53.520 --> 00:54.910
Photoshop very soon.

00:57.470 --> 01:03.650
The top on the list is a big file format depicts transfer joined photographic expert group which was

01:03.650 --> 01:10.680
a committee who invented this file format especially to deal with the smaller cases.

01:10.940 --> 01:17.990
We used to have floppy drive which was 1.4 M-B which is several hundred or thousand times smaller than

01:17.990 --> 01:21.190
the SD card you have on your mobile phone.

01:21.410 --> 01:27.410
And the most commonly used hard drives 20 years back used to be when it was there and we started working

01:27.410 --> 01:31.270
on Photoshop and we realized that we need a lot of bisquits.

01:31.550 --> 01:38.000
That was a time when we used to get the most commonly used or commonly available hardware used to be

01:38.030 --> 01:45.800
1.2 G-B and you can compare that to today's hard drives standard which is the commonly used to this

01:45.800 --> 01:49.880
commonly used harddrive on your computer is at least one terabyte.

01:49.880 --> 01:56.900
That is one TV One Duby is equal to 1024 G-B nothing can compare to the standards today and standard

01:57.080 --> 01:58.150
in those days.

01:58.190 --> 02:02.300
Google you have at least one terabyte hard drive on any computer.

02:02.450 --> 02:09.250
And in those days the limitation was of 1.2 G-B or so and it was obvious that something like just big

02:09.260 --> 02:10.300
was required.

02:10.730 --> 02:17.090
And therefore Gippi came into existence and even became the most popular file format for the images

02:17.370 --> 02:21.330
now depict is not invented before the show but it is not related to Photoshop.

02:21.530 --> 02:28.880
Budget big was invented much before the show was released in the market DP point format is also known

02:28.880 --> 02:35.540
for its quality loss and it is known as a lossy file format but then the standards have reached a level

02:35.540 --> 02:38.480
where you dont have to worry about the loss of quality.

02:38.480 --> 02:44.750
If you save a big file with 100 percent quality it will retain the important elements of the image and

02:45.020 --> 02:53.070
the quality elements of the image and it can give you the best quality of images in all possible ways.

02:53.090 --> 03:00.200
Therefore a good big NO is the most commonly used find format for everything for websites who don't

03:00.200 --> 03:01.750
have any other option but Gippi.

03:01.820 --> 03:10.580
So the images you see on the Web sites ranging from small buttons to the promotional images and the

03:10.580 --> 03:11.180
banners.

03:11.240 --> 03:14.460
Everything is in deep file format as well as youth.

03:14.540 --> 03:20.010
You can use Gippi file format for printing glossy brochures magazines and all other things.

03:20.060 --> 03:28.200
So a wide range of usage Ribbeck file format without anybody about the quality loss of images.

03:28.670 --> 03:32.750
The next commonly used file format is diff Dagh information file format.

03:33.040 --> 03:40.050
Unlike g it does not compress the quality of the images but it does compress the file size of the images

03:40.100 --> 03:41.790
and that's the advantage.

03:41.810 --> 03:48.830
The file size file size and defined format are not smaller like TPD the file size is still huge.

03:49.010 --> 03:54.750
But then the advantage is that like DP It does not touch the quality of images.

03:54.750 --> 04:02.690
Now as I explained the big standards have raised about the expectation and it can retain the quality

04:02.690 --> 04:03.510
of the image.

04:03.650 --> 04:10.460
But then there are some technical differences of which only the file formats can have and cannot handle

04:10.460 --> 04:13.360
that which I'll explain you in the next video.

04:13.550 --> 04:20.950
Default format is usually used for printing jobs very high quality printing is required.

04:20.960 --> 04:25.690
The file file formats of files are saved in diff file format

04:28.410 --> 04:36.180
Notty file formats have the advantage which is the possibilities of saving less or editable less in

04:36.180 --> 04:37.160
Photoshop meaning.

04:37.170 --> 04:39.910
Let me explain you with this image.

04:39.960 --> 04:46.830
I have two layers in this image and you might not understand what is less but then Lears is the one

04:46.830 --> 04:48.930
of the most important topics in this.

04:48.930 --> 04:52.470
So we'll see layers later in the sports.

04:52.510 --> 05:00.650
But right now you just need to see this small demo of Lares is that we have two layers in this image.

05:00.810 --> 05:08.190
The image of the fish is superimposed with the help of LEDs and this file no can be saved as if file

05:08.190 --> 05:12.030
form in the file format and that's the advantage of the file format.

05:12.030 --> 05:14.340
This cannot be done with the JPEG file format.

05:14.520 --> 05:20.610
The big file format cannot have Lares and motorboating file format in the next video will see the next

05:20.610 --> 05:21.210
file format.

05:21.210 --> 05:29.200
We are going to look at is B S D that is Photoshop document and it is for the shops on Adobe Photoshop.

05:29.220 --> 05:35.220
On file format we do editing work in the file format and saved those editable files and because the

05:35.220 --> 05:42.620
file format when we need output or we need to use the image on website or print being or anywhere else.

05:42.660 --> 05:49.980
We save that image as a big meaning we literally can word that image and project file format but to

05:49.980 --> 05:51.350
work or edit that image.

05:51.360 --> 05:57.840
We retain BSD file format which is the editable file format of Adobe Photoshop.

05:57.840 --> 06:06.780
The important file format we deal with is B and D stands for portable network graphics and this is again

06:06.780 --> 06:13.060
useful for the graphics and we don't use Binjie for printing.

06:13.320 --> 06:17.590
Even if we use DNG for printing it is rare.

06:17.790 --> 06:23.760
The format has but one advantage is that it can have a transparent background meaning.

06:23.940 --> 06:32.400
If I print this or if I put this image on some web page or web site or mobile application this will

06:32.400 --> 06:37.380
be in rectangular Square for a rectangle or square format.

06:37.590 --> 06:40.830
But the Binjie file can have

06:44.140 --> 06:50.690
it don't shape like this and the rest of the area will be transparent or it can have it can even have

06:54.000 --> 06:59.270
some shape like this which other file formats cannot have.

06:59.490 --> 07:03.740
And we can see on the Web site we can see the background in this area.

07:03.900 --> 07:12.040
So Biondi is a transport and file format and will be working with all these file formats quite often

07:12.360 --> 07:17.840
in the schools and you get to know more things about these file formats.

07:17.910 --> 07:23.790
And I'll also try to include as many file formats as possible during this course.
